Precision magnetometry using NV centres	in diamond	

Supervisor 
Paul Stanwix www.uwa.edu.au/people/paul.stanwix (pstanwix@physics.uwa.edu.au)
	   	   	  
The  Nitrogen‐Vacancy (NV)	 centre	 has  recently  emerged  as  a  versatile  tool  for  magnetic  resonance,	 quantum optics,  precision	measurement  and  quantum  information processing. The NV centre is a localized impurity in diamond, consisting of a nitrogen substitutional atom close to a vacancy. It stands out among solid‐state systems because of  the exceptional coherence  properties of its	 electronic spin, which can be  efficiently  prepared,  manipulated  and  measured  using  optical	 and  microwave  excitation, even at room‐temperature.	

A new magnetic field sensing modality has recently been demonstrated, based on single  NV centres in diamond [1]. In collaboration with groups from Harvard and MIT, we aim  to develop ultra‐high sensitivity magnetometers based on this technique, using  ensembles of NV centres in bulk diamond. This honours project will involve the  development  of  a  new  experimental  apparatus	 for  investigating  the  coherence  properties of high-density ensembles of NV centres, and	 for testing new methods for  optimal detection of NV	electron spin ensembles. If you have any questions please don’t hesitate to contact me via the email addres  above.
[1] J.R.	 Maze	et al. “Nanoscale magnetic sensing with an individual electronic spin in diamond”, Nature 455, 644‐8 (2008).